// details in arcs
FN=40;

// a bit thicker lines for dimensions
DIM_LINE_WIDTH = 1;

// plank dimensions
// best to err on the too thick side, thats easier to correct with a plane
plankthick = 19;

// depends on the bird you're making the nestbox for
// 28 = blue tit (pimpelmees)
// 32 = great tit (koolmees)
holediameter = 32;

// used to lock the hinging side
picturehookdiameter = 3;
lockplay = 1;

// keyhole to hang the nest box
keyholediameter = 6;
keyholeslotwidth = 3;
keyholeslotlength = 15;

// roof overhang
overhang = 40;

// cutout size for drainage
drainage = 10;

// for a cuttingplan we need to know the kerf the blade will make
bladewidth = 2.8;

// should not need to touch these values
bottomtohole = 195;
nestwidth = 120;
